PI

B

VACUUM TOWER

Wet leg

(Diesel)

100% ---------------

0% -------------------

DP Transmitter

HI

LO

A