HOW TO IMPORT FILES FROM ValveLink Mobile 
NOTE: After each test run with ValveLink Mobile, you will see “WRITING EXPORT FILES”  displayed in the upper right corner of the 475 screen. These files can be accessed: 
1. from the Utilities folder in ValveLink Mobile
2. via the Wireless Transfer Utility in ValveLink Mobile
3. from the system card in the 475 Field Communicator
Open AMS Device Manager (the following is from AMS Device Manager Books Online):
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[bookmark: _GoBack]You will have to do this for each test run. After the tag is created in AMS Device Manager (if it didn’t already exist) select Merge for the subsequent files imported.
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First create an export file in Solo. After creating the export file, JISgq it into AMS Device Manager by right-clicking th
Plant Database icon in Device Connection View and selecting mﬁmﬂ alveLinkfitey

The YEIMEMITENTTIN operation brings the valve devices into the database, but it does not put them into levels of the
Plant Locations hierarchy. The Wﬁm devices are visible only in the Device List. You can put the devices into Control Modules
in the Plant Locations hierarchy as desired.

See the Software documentation for information regarding what data is exported.

Note

There are some device parameters that exist in AMS Device Manager but not in AMS EIYRAR software; when you view the
configuration for a device a AMS [ETIIEATE system, the values for these parameters may be blank.




